{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["010_main"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"010_main","index":0,"n_rows":103,"n_cols":7,"rows_kept":103,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Wireless Sender Box BOM",null,null,"(1/9)"]
[]
["No.","ITEM","MANUFACTURE","PARTS","SIZE","QTY","REMARK"]
[1,"CAP-CERAMIC",null,"0.01uF",1608,2]
[2,"CAP-CERAMIC",null,"0.1uF",1005,211]
[3,"CAP-CERAMIC",null,"22pF",1608,8]
[4,"CAP-CHEMICAL",null,"100uF(16V)","SMT",1]
[5,"CAP-CHEMICAL",null,"100uF(6.3V)","SMT",2]
[6,"CAP-CHEMICAL",null,"10uF(10V)","SMT",6]
[7,"CAP-CHEMICAL",null,"10uF(36V)","SMT",1]
[8,"CAP-CHEMICAL",null,"1uF(16V)","SMT",1]
[9,"CAP-CHEMICAL",null,"4.7uF(25V)","SMT",1]
[10,"CAP-CHEMICAL",null,"4.7uF(50V)","SMT",1]
[11,"CAP-CHEMICAL",null,"UWT1V331MNR","SMT",1]
[12,"CAP-FILM",null,"100pF (3kV)","AXIAL",1]
[13,"CAP-OS",null,"16FP270M","AXIAL",1]
[14,"CAP-TANTALIUM",null,"3.3uF(16V)","SMT",4]
[15,"CON","3M","7614-6002","AXIAL",1]
[16,"CON","AMP","RJHS-5381","AXIAL",1]
[17,"CON","HIROSE","HIF3FC-10PA-2.54DSA","AXIAL",3]
[18,"CON","HIROSE","HIF3FC-14PA-2.54DSA","AXIAL",1]
[19,"CON","HIROSE","IC11SA-68PL-1.27SF-EJR","SMT",1,"with frame"]
[20,"CON","HIROSE","MI20-50PD-SF","SMT",1]
[21,"CON","MAC8","HK-1-G","SMT",1]
[22,"CON","NICHIATSU","B6B-EH","AXIAL",1]
[23,"CON","SMK","LPR6520-0804","AXIAL",7]
[24,"CON","SMK","S-G9312#01","AXIAL",1]
[25,"CON",null,"17LE-23090-D3AB","DB9female",1]
[26,"CON",null,"DIN4","AXIAL",2]
[27,"DIODE","RENESAS","HZU6.2Z","SMT",11]
[28,"DIODE","ROHM","RB051L-40","AXIAL",1]
[29,"DIODE","VTEL","BZG03C16","SMT",1]
[30,"DIODE",null,"1N5820","AXIAL",1]
[31,"DIODE",null,"1SS226","SMT",11]
[32,"IC","ALTERA","EPM3032ALC44-10","QFP",1]
[33,"IC","ALTERA","EPM3064ALC44-10","QFP",1]
[34,"IC","ALTERA","EPM3064ATC100-10","QFP",1]
[35,"IC","CIRRUS","CS4334","SOP",1]
[36,"IC","CIRRUS","CS4954","QFP",1]
[37,"IC","CYPRESS","CY2305","SOP8",2]
[38,"IC","FUJITSU","MBM29DL640E90TN","SOP",2]
[39,"IC","ICSI","IC42S81600-7T","SOP",4]
[40,"IC","MAXIM","MAX3232CSE","SOP",1]
[41,"IC","MAXIM","MAX811SEUS","SMT",1]
[42,"IC","MICRON","MT48LC2M32B2TG-6","SOP",2]
[43,"IC","NS","LM1117MPX-ADJ","SMT",3]
[44,"IC","NS","LM2596S-ADJ","SMT",1]
[45,"IC","PHILIPS","SAA7115HL","QFP",1]
[46,"IC","PHILIPS","UDA1342TS","SOP",1]
[47,"IC","REALTEK","RTL8139C","QFP",1]
[48,"IC","RENESAS","HD6417751RF240","QFP",1]
[49,"IC","ROHM","BR24L04F-W","SOP8",1]
[50,"IC","TI","PCI1510","QFP",1]
[51,"IC","TI","SN74LV541ANS","SOP",2]
[52,"IC","TI","TPS2211APWP","SOP",1]
[53,"IC","TOSHIBA","TC4027BF","SOP",1]
[54,"IC","TOSHIBA","U1GC44","SMT",3]
[55,"IC","VWEB","VW2010","BGA",1]
[56,"IC",null,"AT93C46","SMT",1]
[57,"IND","MURATA","BLM31P500SPT","SMT",2]
[58,"IND","MURATA","BLM31PG500SN1L","SMT",8]
[59,"IND","MURATA","BLM41P600S","SMT",1]
[60,"IND","MURATA","LQH1N2R2K04","SMT",2]
[61,"IND","MURATA","LQH31NR39K01L","SMT",1]
[62,"IND","PULSE","PE-54041-S","SMT",1]
[63,"LED",null,"551-0207","AXIAL",3]
[64,"RES",null,0,1608,14]
[65,"RES",null,10,1608,5]
[66,"RES",null,18,1608,4]
[67,"RES",null,20,1608,1]
[68,"RES",null,22,1608,55]
[69,"RES",null,33,1608,3]
[70,"RES",null,50,1608,3]
[71,"RES",null,56,1608,4]
[72,"RES",null,75,1608,7]
[73,"RES",null,100,1608,6]
[74,"RES",null,110,1608,1]
[75,"RES",null,220,1608,9]
[76,"RES",null,330,1608,6]
[77,"RES",null,"1.5k",1608,1]
[78,"RES",null,"100(1%)",1608,1]
[79,"RES",null,"10k",1608,93]
[80,"RES",null,"12k",1608,2]
[81,"RES",null,"15k",1608,1]
[82,"RES",null,"1k",1608,25]
[83,"RES",null,"1k(1%)",1608,1]
[84,"RES",null,"2.2k",1608,1]
[85,"RES",null,"2.7k",1608,2]
[86,"RES",null,"3.3k(1%)",1608,2]
[87,"RES",null,"3.9k(1%)",1608,1]
[88,"RES",null,"4.7k",1608,14]
[89,"RES",null,"47(1%)",1608,1]
[90,"RES",null,"56k",1608,2]
[91,"SW","MATSUSHITA","EVQPF003M","SMT",4]
[92,"SW","OMRON","A6S-4104","AXIAL",1]
[93,"TR","TOSHIBA","RN1105","SMT",1]
[94,"TRANS","PULSE","PE-68515L","SMT",1]
[95,"XTAL","FINE CLOCK","AS7-20.000MHz","SMT",1]
[96,"XTAL","FINE CLOCK","AS7-25.000MHz","SMT",1]
[97,"XTAL","FINE CLOCK","DT-38","AXIAL",1]
[98,"XTAL-OSC","FINE CLOCK","ACO-331AP4-27.000MHz","SMT",1]
[99,"XTAL-OSC","FINE CLOCK","ACO-331AP4-33.000MHz","SMT",1]
[100,"XTAL-OSC","KINSEKI","FXO-31F 32.11MHz","SMT",1,"or FINE CLOCK"]