{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":11,"n_cols":7,"rows_kept":11,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["映像・波形合成装置設定一覧"]
[]
["チャンネル","最低電圧[V]","最大電圧[V]","表示数値の最低値","表示数値の最大値","グラフの最大幅[ドット]","備考"]
[1,0,5,0,4.995,100]
[2,0,5,0,4.995,100]
[3,0,5,0,4.995,100]
[4,0,5,0,4.995,100]
[5,0,5,0,4.995,100]
[6,0,5,0,4.995,100]
[7,0,5,0,4.995,100]
[8,0,5,0,4.995,100]